

IMG_256***PJ-B551P-V7L***

**LCD FHD**

**Narrow bezel panel**

**For video wall**

****



|  |  |
| --- | --- |
| **Model No.** | PJ-B551P-V6L |
| **View Area(L\*H) (mm)** | 1209.6\*680.4 |
| **Outer case size(mm)** | 1210.51×681.22×123mm |
| **N.W.(kgs/unit)** | 28.8 |
| **Panel specifications** | |
| **Panel Size** | **55inch** |
| **Backlight** | LED |
| **LCD panel Brand** | **LG** |
| **Panel No** | **LD550DUN-TMA4** |
| **Brightness** | 500cd/m2 |
| **bezel for combined two panels** | 0.88mm |
| **Contrast Ratio** | 1100 : 1 |
| **Resolution** | 1920\*1080 |
| **Viewing Angle** | 178°/178°(H,V) |
| **Color** | 10Bit (D), 1.07 Billion colors. 72% NTSC |
| **Response Time** | 8ms |
| **Refresh Rate** | 60Hz |
| **Using life** | 50,000(hrs) |
| **Power** | |
| **Power supply** | AC100V-240V, 50/60Hz |
| **Max Power consumption** | 170W |
| **Standby power consumption** | 0.5W |
| **Video wall controller( Built in each screen)** | |
|  | |
| **DVI in** | 1 (MAX 1920 X 1080 @60 HZ input support) |
| **HDMI in** | 1 (MAX 3840 X 2160 @30 HZ input support) |
| **VGA in** | 1 (MAX 1920 X 1080 @60 HZ input support) |
| **AV in** | 1(BNC, NTSC, PAL support) |
| **USB** | 1 |
| **RS232 In** | 1 |
| **RS232 Out** | 2 |
| **Control signal input and loop out** | RS232 In&Out |
| **Control interface** | remote controller or RS232 |
| **Video system** | |
| **Color system** | PAL/NTSC/SECAM |
| **3D comb filter and video comb filter** | Yes |
| **OSD Language** | English Chinese; (to be available in multiple languages) |
| **Temperature** | |
| **Working temperature** | 0 ℃ ~ 50 ℃ (no condensation) |
| **Working humidity** | 10% ~ 90% (no condensation) |
| **Accessories** | |
| User Manual ,power cable,, RJ45 cable, IR receiver, remote controller, HDMI/DVI cable, USB-RS232 converter, RS232 to RJ45 converter | |
| **Partner with** | |
| 国家高新技术企业 (1)23 | |
| **Real Picture** | |
|  | |
| **Project Pictures** | |
|  | |