

**YXDXXHD-WD**

**Indoor Ceiling Mount Single Sided**

**2500nits Digital Window Display**



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Panel Size** | **43inch** | **49inch** | **55inch** | **65inch** | **75inch** |
| **Model No.** | YXD43HD-WD | YXD49HD-WD | YXD55HD-WD | YXD65HD-WD | YXD75HD-WD |
| **LCD specification** | | | | | |
| **Active Area** | 941.18×529.42 | 1073.78×604 | 1209.6×680.4 | 1428.5×803.5 | 1650\*928mm |
| **Contrast ratio** | 1200:1 | 1200:1 | 1400:1 | 1400:1 | 1400:1 |
| **Resolution** | 1920\*1080/3840\*2160 | 1920\*1080/3840\*2160 | 3840\*2160 | 3840\*2160 | 3840\*2160 |
| **Brightness** | 2500cd/m2 (3000cd/m2 high TNI panel is optional) | | | | |
| **Direction** | Vertical/horizontal optional | | | | |
| **Color** | 16.7M | | | | |
| **Viewing angle** | 178/178 | | | | |
| **LED backlight** | Yes | | | | |
| **Display mode** | Landscape or portrait mode are optional | | | | |
| **Response time** | 8ms | | | | |
| **Life** | 50000(hrs) | | | | |
| **Hardware Specification** | | | | | |
| **CPU** | RK3568 | | | | |
| **Memory** | 2GB | | | | |
| **Nand flash** | 16GB | | | | |
| **Storage port** | USB, SD card | | | | |
| **OS** | **Android 11** | | | | |
| **WiFi** | Yes, inbuilt WiFi(802.11b/g/n); 4G optional | | | | |
| **Power** | | | | | |
| **Power supply** | 90-132VAC/180-264VAC(Select by the transfer switch) | | | | |
| **Operation temperature** | 0℃-60℃ (no condensation) | | | | |
| **Operation humidity** | 10%-85% (no condensation) | | | | |
| **System function** | | | | | |
| **Support video** | MPEG1/MPEG2/MPEG4/AVI/VOB/MOV/WMV/DIVX/RM/RMVB, support super HD 1080P/2160P video | | | | |
| **Support picture** | JPG/JPEG/PNG/BMP | | | | |
| **Support TXT** | TXT/WORD/EXCEL/PDF | | | | |
| **Support Website** | HTML/ASP/JSP/PHP | | | | |
| **Support RSS** | Internet RSS title and text, flip over/page turning | | | | |
| **Long-distance control** | monitoring the terminal display image in real time | | | | |
| **Image rotate** | support 90°,180°,270°image rotate | | | | |
| **Software upgrade** | Support upgrade software by USB disk | | | | |
| **Structure** |  | | | | |
| **Install method** | Ceiling Mounting/Wall Mount | | | | |
| **Color** | Black | | | | |
| **Speaker** | Built-in speaker is optional | | | | |
| **Brightness sensor** | Yes, built-in | | | | |
| **Working Time** | 7\*24hours | | | | |
| **Pictures** |  | | | | |
|  | | | | | |
| **Dimension** | | | | | |
| **43inch:**    **49inch:**    **55inch:**    **65inch:**    75inch | | | | | |